Start On low power

Turn coarse adjustment to lower all the way

Center fine adjustment knob

Check diaphragm--open to let in most light

Check mirror-- turned correctly

**ONLY USE COARSE ADJUSTMENT ON LOW POWER**